DATE: 2025-07-01

ATTN: Quote #: Q-1003

Subject:

1 QTY LS2000 $675.00 EACH

* Supply Voltage:
* Output: 10 Amp SPDT Relay
* Selectable Fail-Safe High or Low Level
* Process Connection: , (300 PSI Max.)
* Insulator: Teflon, 4” Long (450 F)
* Probe: ½” Diameter HALAR x XX” (Including Insulator)
* Housing: Cast Aluminum, NEMA 7, C, D; NEMA 9, E, F, & G
* 2-Year Warranty

Notes:

* For longer probes please add $ 110.00 per foot
* Other supply voltages available at no extra charge
* Special materials of construction – please call factory

Delivery: FOB; Houston, TX

Terms: NET 30 W.A.C. Quotation valid for 30 days.

Please contact me directly if you have any questions or require more information.

Thank you,

Sales Representative

(555) 987-6543

quotes@babbitt.com

[www.babbittinternational.com](http://www.babbittinternational.com/)